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MANUAL MODEL
Suggested Architectural Specifications
Section 8


Model GT1500
Aluminum Sliding Service Window System

Division 08 – Openings
Section 08 56 59 SERVICE WINDOW UNITS

Note to Specifier: Articles and paragraphs below may be edited or modified to suit specific project requirements.  

Add section numbers and titles per CSI “MasterFormat” and specifier’s standard practice.  Contact manufacturer’s representative to discuss specification modifications, performance requirements, accessories and/or related equipment that may be applicable to this project. 

Part 1 - GENERAL

1.01 DESCRIPTION
A. Furnish and install manual slide door equipment as indicated on drawings and specifications.

B. Related work specified elsewhere.

1. Concrete: Division 03, applicable sections.
2. Masonry: Division 04, applicable sections.
3. Thermal and Moisture Protection: Division 07, applicable sections.
4. Openings: Division 08, applicable sections.

1.02 REFERENCES
A. American National Standards Institute (ANSI) - www.ansi.org
B. Builders’ Hardware Manufacturers Association (BHMA) - www.buildershardware.com
C. Underwriters Laboratory, Inc. (UL) - www.ul.com

1.03 QUALITY ASSURANCE
A. Manufacturer’s Qualifications: Manufacturer to have at least (5) five years of experience in the fabrication of automatic and manual entrance systems.

B. Installer’s Qualifications: Products specified shall be represented by a factory authorized and trained distributor. Distributor shall be AAADM Certified, maintain a parts inventory and have trained service personnel with experience installing and maintaining units indicated for this project.

C. NABCO equipment as manufactured by NABCO ENTRANCES, INC. has been specified and shall be quoted as a base bid.  

1.04 SUBMITTALS
A. Submit listed submittals in accordance with Conditions of the Contract and Division 1 Specifications Section. 

B. Shop Drawings: Submittal drawings, templates and/or diagrams showing layout, anchorage, accessories and glazing details shall be furnished to fabricators and installers of related work for coordination of sliding window system with concrete work, electrical work, and other related work (where required).

C. Closeout documents:  
a. A copy of owner’s manual shall be provided to owner’s representative upon completion of installation. 
b. Warranties

1.05 SUBSTITUTIONS 
A. Equipment as manufactured by NABCO Entrances, Inc. has been specified and shall be quoted as the base bid. Proposals for substitution products may be submitted by the bidding contractors a minimum of 10 days prior to bid due date. The proposed substitution shall meet the quality and performance standards described in this specification. 

1.06 JOB SITE CONDITIONS
A. Site Survey: Verify site conditions including, but not limited to the following; opening sizes, floor conditions, plumb and level mounting surfaces (substrates shall be of proper dimension and material). 

B. Coordinate installation with glass, glazing, hardware and other trades to avoid construction delays.

1.07 WARRANTY
A. Warranted materials shall be free of defects in material and workmanship for a period of one year from date of substantial completion. During the warranty period the Owner shall request NABCO factory-trained technicians to perform service.  Warranty repairs are provided during normal business hours.  Owner to receive warranty after completion of installation.

PART 2-PRODUCTS

2.01 APPROVED MANUFACTURER
A. All door equipment shall be manufactured by:
NABCO Entrances Inc.
[bookmark: _Hlk55205694]S82 W18717 Gemini Drive
Muskego, WI 53150
Phone: (877) 622-2694
Fax: (888) 679-3319
Email: info@nabcoentrances.com

NABCO Entrances, Inc., shall manufacture automatic and/or manual service window(s) of type(s) and size(s) specified on plans and window schedules.

2.02 CONVENIENCE WINDOW
Model GT 1500 Convenience Window as indicated on window schedule and details.

A. Types / Configurations: 
1. GT 1500-01L-M (O-X): Manual Single Left-Hand Slide, viewed from exterior.
2. GT 1500-01R-M (X-O): Manual Single Right-Hand Slide, viewed from exterior.
3. GT Model 1500-02-M - (O-X-X-O): Manual Bipart Sliding, viewed from exterior.

B. Product Components:
1. Aluminum window(s), sidelite(s), operator housing and frame.
2. Rollers-support, anti-rise and guide.
3. Window carrier hanger assembly (non-breakout)
4. Air infiltration and intrusion protection equipment.

1a) Horizontal Header shall be 5” x 4-1/2” (127mm x 114mm) extruded aluminum with end caps.  Header shall be accessible by hinged cover that locks in the open position for ease of service. 
1b) Window panel(s) and sidelite(s) panel shall be factory assembled using 3/8"-16 threaded tie rods spanning full length of top and bottom rails. Snap-in glass stop with integral extruded vinyl standoff to accommodate glass flexing. Narrow stile 2-1/8” (51mm). 
1c) Sidelite configuration shall be fixed sidelite.
1d) Vertical jambs on “Manual” units shall be 1-3/4” x 4-1/2” (44mm x 114mm) extruded aluminum tubes. Vertical jambs on “Automatic” units shall be (1) one 2” x 5” (51mm x 127mm) and (1) one 3 1/2” x 5” (89mm x 127mm) extruded aluminum tubes.

2a) The window assembly shall ride on two steel, urethane coated support rollers, incorporating lubricated sealed ball bearings.  The window shall be held on the track by means of two equivalent anti-rise rollers. Lateral adjustment of the window assembly shall provide positive sealing at window edges.  Window height adjustment - each roller assembly shall have ± 7/16” (11mm) of vertical adjustment
2b) Fixed Sidelite - Each window shall include one bottom mounted fixed guide assembly.  Guide not to be subject to corrosion or effects of weather. Material to be Delrin or equivalent.

3a) Convenience window systems shall have window panel(s) attached to a solid aluminum window carrier hanger assembly by means of mechanical fasteners to prevent breakout or forced entry of the sliding panel.
3b) The active window will incorporate a hook bolt lock with multi-ply construction and hacksaw resistant center core for securing the lead stile(s).  In the case of a single slide, the window is secured at the jamb.  The lock assembly will incorporate a thumb turn on the interior.

4a) Double pile weather-stripping on the lead edge of the sliding window(s) .36" thick (9mm) including the area of the lock.
4b) 9/16" (14mm) wide nylon brush weather-stripping on the vertical stile of both the sliding window panel(s) and sidelite(s) panels
4c) 15/16" (24mm) wide nylon brush weather-stripping mounted on window bottom.

2.04 MATERIALS, FINISHES AND FABRICATION
A. All extruded aluminum sections shall be 6063-T5 or equivalent. 
B. Finish:  Aluminum shall have a standard finish of AA-M12-C22-A31 (204R1, clear) or AA-M12-C22-A44 (dark bronze).
C. Special Anodize: Colors available upon request.
D. Special Paint: Colors available upon request.
E. Special Clad: Stainless or muntz metal (polished or satin finish) available upon request.

PART 3-EXECUTION

3.01 EXAMINATION

Site Survey: Installer shall field verify site conditions to ensure that the product can be installed according to the manufacturer’s instructions. Notify the Contractor in writing of any conditions that are deemed to be unacceptable for proper and timely completion of work. Do not begin installation until negative conditions are corrected in a manner acceptable for the proper installation of the product.  

3.02 INSTALLATION
A. GENERAL: GT 1500 Convenience Window shall be installed by factory trained installers in compliance with manufactures recommendations and approved shop drawings. Units will be installed plumb and level, without warping or racking of frames or sash within the manufacturers prescribed tolerances. Provide proper support and anchor in place. 
B. DISSIMILAR MATERIALS: Provide separation of aluminum materials and other corrodible surfaces from sources of corrosion or electrolytic action contact points by complying with AAMA 101, Appendix, titled “Dissimilar Materials”.
C. WEATHER-TIGHT CONSTRUCTION: Install header, jambs and sill members in a bed of sealant or with joint filler or gaskets, to provide weather tight construction. Coordinate installation with wall flashings and other components of construction.

3.02 CLEANING AND PROTECTION
A. After installation, clean framing members as recommended by manufacturer.  Aluminum surfaces in contact with masonry, concrete, or steel shall be protected from contact by use of neoprene gaskets where indicated or a coat of bituminous paint to prevent galvanic or corrosive action.  Advise general contractor to protect unit from damage during subsequent construction activities.

*COVER NOTE TO SPECIFICATION WRITER
A. Preparation of a plumb and square opening to receive sliding door equipment with adequate support.

B. Glass and glazing shall be described in glazing section of the specifications, door to be glazed square.
 
C. CONCRETE INSTALLER shall prepare floor at location of entrance system to be level and smooth without changes in elevation between foundation and associated walkways.

D. CONTRACTOR shall prepare opening(s) at the location(s) of convenience window installation(s) to accommodate the size(s) as indicated on drawings.
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