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INSTALLATION NOTES:

1. THE NUMBER OF INSTALLATION ANCHORS DEPICTED
1S THE MINIMUM NUMBER OF ANCHORS TO BE USED
FOR PRODUCT INSTALLATION.

MINIMUM EMBEDMENT AND EDGE DISTANCE
EXCLUDE WALL FINISHES, INCLUDING BUT NOT
LIMITED TO STUCCO, FOAM, BRICK VENEER, AND
SIDING.

USE TWO (2) INSTALLATION ANCHORS AT EACH
LOCATION SHOWN (SEE SHEETS 2)

FOR INSTALLATION THROUGH 1X BUCK TO
CONCRETE/MASONRY OR DIRECTLY INTO
CONCRETE/MASONRY, USE 1/4 INCH ITW TAPCONS
OF SUFFICIENT LENGTH TO ACHIEVE 1 3/4 INCH
MINIMUM EMBEDMENT INTO CONCRETE/MASONRY.
CONCRETE/MASONRY ANCHORS SHALL MAINTAIN A
MIN. EDGE DISTANCE OF 2 1/2 INCH.

FOR INSTALLATION THROUGH METAL STUD USE
1/4-14 TEK SCREWS OF SUFFICIENT LENGTH TO
ACHIEVE 3 THREADS MINIMUM PENETRATION
BEYOND METAL STRUCTURE. METAL ANCHORS
SHALL MAINTAIN A MINIMUM EDGE DISTANCE OF
3/4 INCH.

INSTALLATION ANCHORS AND ASSOCIATED
HARDWARE MUST BE MADE OF CORROSION
RESISTANT MATERIAL OR HAVE A CORROSION
RESISTANT COATING.

FOR GROUT FILLED BLOCK, DO NOT INSTALL
INSTALLATION ANCHORS INTO MORTAR JOINTS.
EDGE DISTANCE IS MEASURED FROM FREE EDGE OF
BLOCK OR EDGE OF MORTAR JOINT INTO FACE SHELL
OF BLOCK.

INSTALLATION ANCHORS SHALL BE INSTALLED IN
ACCORDANCE WITH ANCHOR MANUFACTURER'S
INSTALLATION INSTRUCTIONS, AND ANCHORS SHALL
NOT BE USED IN SUBSTRATES WITH STRENGTHS LESS
THAN THE MINIMUM STRENGTH SPECIFIED BY THE
ANCHOR MANUFACTURER.

INSTALLATION ANCHOR CAPACITIES FOR PRODUCTS
HEREIN ARE BASED ON SUBSTRATE MATERIALS WITH
THE FOLLOWING PROPERTIES:

A. CONCRETE -MINIMUM COMPRESSIVE STRENGTH
OF 3192 PSI.

B. MASONRY - STRENGTH CONFORMANCE TO ASTM
C-90, GRADE N, TYPE 1 (OR GREATER).

C. GROUT-FILLED CMU - UNIT STRENGTH CONFORMS
TO ASTM C-90 WITH MINIMUM COMPRESSIVE
STRENGTH OF 2000 PSI AND GROUT CONFORMS
TO ASTM C 476, MINIMUM GROUT COMPRESSIVE
STRENGTH OF 2000 PSI.

. HOLLOW BLOCK CMU - UNIT STRENGTH
CONFORMS TQ ASTM C-90 WITH MINIMUM
COMPRESSIVE STRENGTH OF 2000 PSI.

. STEEL - MINIMUM 1/8 INCH A36 STEEL

. ALUMINUM - MINIMUM 1/8 INCH 6063-T5
ALUMINUM

NABCO

SYSTEM GT 1400 - AUTOMATIC ALUMINUM
BIFOLD GLASS DOOR (IMPACT)
(FS-FX-FX-FS)

GENERAL NOTES:

1.

THE PRODUCT SHOWN HEREIN IS DESIGNED AND
MANUFACTURED TO COMPLY WITH THE 5TH EDITION
(2014) FLORIDA BUILDING CODE (FBC), INCLUDING HVHZ.

o TAS 201-94

o TAS 202-94

» TAS 203-94

ADEQUACY OF THE EXISTING STRUCTURAL
CONCRETE/MASONRY AND 2X FRAMING AS A MAIN WIND
FORCE RESISTING SYSTEM CAPABLE OF WITHSTANDING
AND TRANSFERRING APPLIED PRODUCT LOADS TO THE
FOUNDATION IS THE RESPONSIBILITY OF THE ENGINEER OR

ARCHITECT OF RECORD FOR THE PROJECT OF INSTALLATION.

1X AND 2X BUCKS (WHEN USED) SHALL BE DESIGNED AND
ANCHORED TO PROPERLY TRANSFER ALL LOADS TO THE
STRUCTURE. BUCK DESIGN AND INSTALLATION IS THE
RESPONSIBILITY OF THE ENGINEER OR ARCHITECT OF
RECORD FOR THE PROJECT OF INSTALLATION.

THE INSTALLATION DETAILS DESCRIBED HEREIN ARE
GENERIC AND MAY NOT REFLECT ACTUAL CONDITIONS FOR
A SPECIFIC SITE. IF SITE CONDITIONS CAUSE INSTALLATION
TO DEVIATE FROM THE REQUIREMENTS DETAILED HEREIN,
A LICENSED ENGINEER OR ARCHITECT SHALL PREPARE SITE
SPECIFIC DOCUMENTS FOR USE WITH THIS DOCUMENT, IN
NON HVHZ AND TO BE REVIEWED BY BUILDING OFFICIAL.
FOR HVHZ DEVIATION FROM APPROVAL REQUIRES ONE
TIME APPROVAL FROM MIAMI-DADE COUNTY (PERA).

APPROVED IMPACT PROTECTIVE SYSTEM IS NOT REQUIRED
ON THIS PRODUCT IN AREAS REQUIRING IMPACT
RESISTANCE.

DOOR FRAME MATERIAL: ALUMINUM 6063-T6 UNLESS
OTHERWISE NOTED.

DISSIMILAR METALS INCLUDING FASTENERS THAT MAY
COME INTO CONTACT WITH ALUMINUM UNIT FRAMING
SHALL BE PROTECTED AS DEFINED IN THE FBC.

GLASS SHALL MEET THE REQUIREMENTS OF ASTM E1300-04
GLASS CHARTS. SEE SHEET 6 FOR GLAZING DETAILS.

DESIGNATIONS "FX" AND "FS" STAND FOR THE FOLLOWING:
FX: OPERABLE BREAKOUT PANEL
FS:  FIXED SWINGING PANEL
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TYPICAL CLUSTER OF 96" MAX.
2 PAIRS OF ANCHORS
SPACED AT 8"OC

TYPICAL CLUSTER OF
1PAIR OF ANCHORS
AT EACH TOP CORNER

91.50" MAX.

14 ANCHORS SINGLE ROW

96" MAX.

72-1/2 NET
DOOR OPENING
——

84-1/4" FULL
BREAK-OUT OPENING

ELEVATION

INTERIOR VIEW
(FS-FX-FX-FS)

NOTE:

SEE SHEET 1, INSTALLATION NOTES 5 & 6
FOR ANCHOR TYPE AND INSTALLING
REQUIREMENTS.

TYPICAL CLUSTER OF
2 PAIRS OF ANCHORS
SPACED AT 8"'0C

TYPICAL CLUSTER OF
1PAIR OF ANCHORS
AT EACH TOP CORNER

50.50" MAX.

ANCHORS INTO
TWO ROWS 91.50" MAX.
SPACED AT 12"0C

INTERIOR INTERIOR

l ANCHORS INTO TWO ROWS

SPACED AT 12"0C

= SINGLE ROW

7 ANCHORS

50.50" MAX. ———

36-1/4"

NET DOOR —
OPENING

"FSFX" OR "FXFS"

42-1/8" FULL
BREAK-OUT —=|
OPENING

ELEVATION

INTERIOR VIEW
(FSFX OR FXFS)

MANUFACTURER:

NABCO

GYRO TECH
$82 W18717 GEMIN| DRIVE
P.O. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

DANIA BEACH, FL 33004

ELEVATION & ANCHOR LAYOUT
(954) 399-8478
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DOOR PIVOT

DOOR PIVOT
5/8" TYP. STRIKE STILE END STILE END

ROD ENGAGEMENT \

46" TYP.

KAWNEER #37227
FLUSH BOLTS

ADAMS RITE
LOCK W/ BOLTS

y 4

KAWNEER #37227
FLUSH BOLTS

DOOR PIVOT
DOOR PIVOT STILE END

STRIKE STILE END

DOOR HARDWARE DETAIL

NOTE:

KAWNEER #37227 FLUSH BOLTS MAY BE SUBSTITUTED
W/ADAM'S RITE 1870 CYLINDER ACTIVATED BOLTS, TOP
& BOTTOM.

1/4-20X3/4"
MOUNTING SCREWS

TOP RAIL

-~ 1313

STRIKE STILE END DETAIL

HEADER

OPERATOR DRIVE
SHAFT WELDMENT

GUIDE CHANNEL

1/4-20X3/4"
MOUNTING SCREWS

TOP RAIL

DOOR PIVOT STILE END DETAIL

MANUFACTURER:

NABCO

GYRO TECH

$82 W18717 GEMINI DRIVE
P.0. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

DANIA BEACH, FL 33004

SYSTEM 6T 1400 BIFOLD DOOR
DOOR HARDWARE DETAILS
(954) 399-8478

398 E. DANIA BEACH BLVD. #338

o)
BUILDING DROPS, INC.
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PREPARED BY:
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MAX.DLO
7115/16"

INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

1
T PERIMETER

SEALANT
MAX. 1/4" SHIM

HEADER

EXTERIOR INTERIOR

GUIDE CHANNEL

STOP BLOCK

WEATHERING PILE
(SCHELEGEL POLYBOND)

TOP RAIL

. VERTICAL SECTION

MANUFACTURER:

NABCO

GYRO TECH

$82 W18717 GEMIN| DRIVE
P.0. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

SEE GLAZING
DETAIL SHEET 6

$

MAX.DLO
7115/16"

VERTICAL SECTIONS
DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM GT 1400 BIFOLD DOOR

TITLE:
PREPARED BY:
0}
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398 E. DANIA BEACH BLVD. #338

EXTERIOR INTERIOR

N
Z
O
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>
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INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

. VERTICAL SECTION
“ SILL

DANIA BEACH, FL 33004

PE CERT. OF AUTHORIZATION NO. 20578

HERMES F. NOREROQ, P.E.
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD.
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INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

WEATHERING BULB

PIVOT STILE END
SEE DETAIL SHEET 3

EDGE
DISTANCE

< E }HORlZONTAL SECTION
MAX. 1/4" SHIM e

INTERIOR

SEE GLAZING AR LOCK W/ BOLTS
DETAIL SHEET 6

LOCK REINF.PLATES
SEE SHEET 7 FOR
DETAILS

WEATHERING BULB

EXTERIOR

E E}HORIZONTAL SECTION
PANEL BUTT STILE

MANUFACTURER:

WEATHERING PILE NABCO
INTERIOR (SCHELEGEL POLYBOND)

GYRO TECH

S82 W18717 GEMIN| DRIVE

HINGE TUBE P.0O. BOX 906 MUSKEGO,
E GLAZING WISCONSIN 53150

KAWNEER TAIL SHEET 6 PHONE: (877) 622-2694
FLUSH BOLTS FAX: (262) 679-2505

(954) 744-4738

HORIZONTAL SECTIONS
BUILDING DROPS, INC.
DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM GT 1400 BIFOLD DOOR

STRIKE STILE
END PIVOT

(SEE SHEET 3 FOR
DETAILS)

398 E. DANIA BEACH BLVD. #338

TITLE:

O)

EXTERIOR

.HORIZONTAL SECTION
v PANEL INTERLOCK

INTERIOR —INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

BY | DATE

WEATHERING BULB

REVISIONS

DESCRIPTION

AR LOCK

A | 5TH EDITION FBC REVISIONS | LS| 9.28.15 | PREPARED BY:

HERMES F, NORERO, P.E,
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD,
DANIA BEACH, FL 33004
BPE CERT. OF AUTHORIZATION NO. 20578

EXTERIOR MAX. 1/4" SHIM

{ E }HORIZONTAL SECTION
JAMB

MTT
CHK BY:
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¢ 0170 ‘_ GUIDE CHANNEL 6063-T5 248913 W.L. BONNEL CO.

BILL OF MATERTIALS

HEADER ITEM NO. DESCRIPTION MATERIAL NABCO PART NO. | MANUFACTURER
6063-T6 HEADER 6063-T6 248912 W.L. BONNEL €O.

WL BONNEL Co.
WL BONNEL CO.
e eme | amwe | wew  [wesowmeco
& [wweson | wews | W0k [wesoweco.
o [Tmesmowmaw | cwoers | @07 lwe soweLco]
WL BONNEL co.
WL BONNEL co.
ve | s | |

1/2" O.A. LAMINATED GLASS CONSISTING OF:
3/16" TEMPERED GLASS

1/8" SOLUTIA SAFLEX PVB INTERLAYER

3/16" TEMPERED 6LASS

EXTERIOR  1/2" INTERIOR
6LASS Y x %" x %" ALUMINUM
REINFORCEMENT ANGLE

GUIDE CHANNEL HEADER DRESS PLATE DOW 995

STRUCTURAL
3-T 3-T!
6063-T5 6063-T5 STLICONE

r 0.320 THREAD FORMING AT 6"OC

——1.810 —= #10-24X1 PFH SCREW
2" FROM ENDS

#10-24X2" PFH SCREW
THREAD FORMING AT 12"0C
GLAZING DETAIL 1 AND 3" OC NEAR THE CORNERS

GLASS THICKNESS AND TYPE COMPLIES WITH
ASTM E 1300-04 GLASS CHART REQUIREMENTS.
ALL GLAZING CONFIGURATIONS SHALL COMPLY
WITH SAFETY GLAZING REQUIREMENTS
OUTLINED IN FBC SECTION 2406.

MAX. DLO = 15 %" x 71'%,"

MANUFACTURER:

NABCO

GYRO TECH
$82 W18717 GEMINI DRIVE
P.0. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (677) 622-2634
FAX: (262) 679-2505

(954) 744-4738

DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM GT 1400 BIFOLD DOOR
B.O.M. COMPONENTS & GLAZING
BUILDING DROPS, INC.
398 E. DANIA BEACH BLVD. #338

TITLE:

0}

9.28.15 | PREPARED BY:

oo

REVISIONS
DESCRIPTION
5TH EDITION FBC REVISIONS

=
I

DANIA BEACH, FL 33004
CERT, OF AUTHORIZATION NO. 29578

HERMES F. NORERO, P.E,
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD,

SCALE:
NTS
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HINGE TUBE
6063-T5

@1.500 —o_

THRESHOLD RAMP
6005-T5

—= 1250 |=—

0.500

?

4" STILE
6063-T6

STILE
6063-T6

|

2.130
J —=|{=—10.090

‘« 1.750 a‘

‘« 1.750 »‘

@ JAMB EXTENSION
6063-T5

‘—— 2.000 ——‘

GLASS STOP CHANNEL
6063-T5

4»‘ ‘% .056 k

IR

1000

TOP & BOTTOM RAIL DOOR e THRESHOLD

6063-T6
0.090 —~{|=—

1

Y

- 1750 =]

GLASS STOP BASE REINF. ANGLE
6063-T5 6061-T6

045 —o||=— 0.750 <—>‘

} -
100
i

6005-T5

@ TRACK PLUG

RPVC

——‘ ‘« 0.560
it

t

1

INTERIOR

AR 4066

THUMBTURN
ADAMS RITE AR 1853A/505
MAXIMUM SECURITY LOCK
EXTENDING INTO HEADER
AND THRESHOLD

LOCK REINFORCEMENT PLATE
11/2X 15" X .105"
12 GAUGE STEEL

AR 4036 CYLINDER

STANDARD LOCK DETAIL

! L

N
0130 J 0.750

INTERIOR

AR 4550
MS DEADBOLT LEVER

ADAMS RITE AR 1853A/505
MAXIMUM SECURITY LOCK
EXTENDING INTO HEADER

AND THRESHOLD

LOCK REINFORCEMENT PLATE
11/2X 15" X 105"
12 6AUGE STEEL

AR 4036 CYLINDER

ALTERNATE LOCK DETAIL

MANUFACTURER:

NAECO

GYRO TECH
582 W18717 GEMIN| DRIVE
P.0. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

SYSTEM 6T 1400 BIFOLD DOOR
COMPONENTS
BUILDING DROPS, INC.
398 E. DANIA BEACH BLVD. #338
DANIA BEACH, FL 33004

(954) 399-8478

0)
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REVISIONS

HERMES F. NORERO, P.E.
FLORIDA P, E. NO, 73778

308 EAST DANIA BEACH BLVD.
DANIA BEACH, FL 33004
PE CERT. OF AUTHORIZATION NO, 29578





