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INSTALLATION NOTES:

1.

THE NUMBER OF INSTALLATION ANCHORS DEPICTED
1S THE MINIMUM NUMBER OF ANCHORS TO BE USED
FOR PRODUCT INSTALLATION.

MINIMUM EMBEDMENT AND EDGE DISTANCE
EXCLUDE WALL FINISHES, INCLUDING BUT NOT
LIMITED TO STUCCO, FOAM, BRICK VENEER, AND
SIDING.

USE TWO (2) INSTALLATION ANCHORS AT EACH
LOCATION SHOWN (SEE SHEETS 2)

FOR INSTALLATION THROUGH 1X BUCK TO
CONCRETE/MASONRY OR DIRECTLY INTO
CONCRETE/MASONRY, USE 1/4 INCH ITW TAPCONS
OF SUFFICIENT LENGTH TO ACHIEVE 1 3/4 INCH
MINIMUM EMBEDMENT INTO CONCRETE/MASONRY.
CONCRETE/MASONRY ANCHORS SHALL MAINTAIN A
MIN. EDGE DISTANCE OF 2 1/2 INCH.

FOR INSTALLATION THROUGH METAL STUD USE
1/4-14 TEK SCREWS OF SUFFICIENT LENGTH TO
ACHIEVE 3 THREADS MINIMUM PENETRATION
BEYOND METAL STRUCTURE. METAL ANCHORS
SHALL MAINTAIN A MINIMUM EDGE DISTANCE OF
3/4 INCH.

INSTALLATION ANCHORS AND ASSOCIATED
HARDWARE MUST BE MADE OF CORROSION
RESISTANT MATERIAL OR HAVE A CORROSION
RESISTANT COATING.

FOR GROUT FILLED BLOCK, DO NOT INSTALL
INSTALLATION ANCHORS INTO MORTAR JOINTS.
EDGE DISTANCE IS MEASURED FROM FREE EDGE OF
BLOCK OR EDGE OF MORTAR JOINT INTO FACE SHELL
OF BLOCK.

INSTALLATION ANCHORS SHALL BE INSTALLED IN
ACCORDANCE WITH ANCHOR MANUFACTURER'S
INSTALLATION INSTRUCTIONS, AND ANCHORS SHALL
NOT BE USED IN SUBSTRATES WITH STRENGTHS LESS
THAN THE MINIMUM STRENGTH SPECIFIED BY THE
ANCHOR MANUFACTURER.

INSTALLATION ANCHOR CAPACITIES FOR PRODUCTS
HEREIN ARE BASED ON SUBSTRATE MATERIALS WITH
THE FOLLOWING PROPERTIES:

A. CONCRETE -MINIMUM COMPRESSIVE STRENGTH
OF 3192 PSI.

B. MASONRY - STRENGTH CONFORMANCE TO ASTM
C-90, GRADE N, TYPE 1 (OR GREATER).

C. GROUT-FILLED CMU - UNIT STRENGTH CONFORMS
TO ASTM C-90 WITH MINIMUM COMPRESSIVE
STRENGTH OF 2000 PSI AND GROUT CONFORMS
TO ASTM C 476, MINIMUM GROUT COMPRESSIVE
STRENGTH OF 2000 PSI.

. HOLLOW BLOCK CMU - UNIT STRENGTH
CONFORMS TQ ASTM C-90 WITH MINIMUM
COMPRESSIVE STRENGTH OF 2000 PSI.

. STEEL - MINIMUM 1/8 INCH A36 STEEL

. ALUMINUM - MINIMUM 1/8 INCH 6063-T5
ALUMINUM

NABCO

SYSTEM GT 1400 - AUTOMATIC ALUMINUM
BIFOLD GLASS DOOR (NON-IMPACT)
(FS-FX-FX-FS)

GENERAL NOTES:

1.

THE PRODUCT SHOWN HEREIN IS DESIGNED AND

MANUFACTURED TO COMPLY WITH THE 5TH EDITION

(2014) FLORIDA BUILDING CODE (FBC), INCLUDING HVHZ.
o TAS 202-94

ADEQUACY OF THE EXISTING STRUCTURAL
CONCRETE/MASONRY AND 2X FRAMING AS A MAIN WIND
FORCE RESISTING SYSTEM CAPABLE OF WITHSTANDING
AND TRANSFERRING APPLIED PRODUCT LOADS TO THE
FOUNDATION IS THE RESPONSIBILITY OF THE ENGINEER OR

ARCHITECT OF RECORD FOR THE PROJECT OF INSTALLATION.

1X AND 2X BUCKS (WHEN USED) SHALL BE DESIGNED AND
ANCHORED TO PROPERLY TRANSFER ALL LOADS TO THE
STRUCTURE. BUCK DESIGN AND INSTALLATION IS THE
RESPONSIBILITY OF THE ENGINEER OR ARCHITECT OF
RECORD FOR THE PROJECT OF INSTALLATION.

THE INSTALLATION DETAILS DESCRIBED HEREIN ARE
GENERIC AND MAY NOT REFLECT ACTUAL CONDITIONS FOR
A SPECIFIC SITE. IF SITE CONDITIONS CAUSE INSTALLATION
TO DEVIATE FROM THE REQUIREMENTS DETAILED HEREIN,
A LICENSED ENGINEER OR ARCHITECT SHALL PREPARE SITE
SPECIFIC DOCUMENTS FOR USE WITH THIS DOCUMENT, IN
NON HVHZ AND TO BE REVIEWED BY BUILDING OFFICIAL.
FOR HVHZ DEVIATION FROM APPROVAL REQUIRES ONE
TIME APPROVAL FROM MIAMI-DADE COUNTY (PERA).

APPROVED IMPACT PROTECTIVE SYSTEM IS REQUIRED ON
THIS PRODUCT IN AREAS REQUIRING IMPACT RESISTANCE.

DOOR FRAME MATERIAL: ALUMINUM 6063-T6 UNLESS
OTHERWISE NOTED.

DISSIMILAR METALS INCLUDING FASTENERS THAT MAY
COME INTO CONTACT WITH ALUMINUM UNIT FRAMING
SHALL BE PROTECTED AS DEFINED IN THE FBC.

GLASS SHALL MEET THE REQUIREMENTS OF ASTM E1300-04
GLASS CHARTS. SEE SHEET 6 FOR GLAZING DETAILS.

DESIGNATIONS "FX" AND "FS" STAND FOR THE FOLLOWING:
FX: OPERABLE BREAKOUT PANEL
FS: FIXED SWINGING PANEL
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P.O. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2604
FAX: (262) 679-2505
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TYPICAL CLUSTER OF 96" MAX.
2 PAIRS OF ANCHORS
SPACED AT 8"OC

TYPICAL CLUSTER OF
1PAIR OF ANCHORS
AT EACH TOP CORNER

91.50" MAX.

14 ANCHORS SINGLE ROW

96" MAX.

72-1/2 NET
DOOR OPENING
——

84-1/4" FULL
BREAK-OUT OPENING

ELEVATION

INTERIOR VIEW
NOTE: (FS-FX-FX-FS)
SEE SHEET 1, INSTALLATION NOTES 5 & 6

FOR ANCHOR TYPE AND INSTALLING
REQUIREMENTS.

TYPICAL CLUSTER OF
2 PAIRS OF ANCHORS
SPACED AT 8"'0C

TYPICAL CLUSTER OF
1PAIR OF ANCHORS
AT EACH TOP CORNER

50.50" MAX.

ANCHORS INTO
TWO ROWS 91.50" MAX.
SPACED AT 12"0C

INTERIOR INTERIOR

l ANCHORS INTO TWO ROWS

SPACED AT 12"0C

= SINGLE ROW

7 ANCHORS

50.50" MAX. ———

36-1/4"

NET DOOR —
OPENING

"FSFX" OR "FXFS"

42-1/8" FULL
BREAK-OUT —=|
OPENING

ELEVATION

INTERIOR VIEW

(FSFX OR FXFS)

MANUFACTURER:

NABCO

GYRO TECH

882 W18717 GEMINI DRIVE
P.O. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

BUILDING DROPS, INC.
398 E. DANIA BEACH BLVD. #338
DANIA BEACH, FL 33004

ELEVATION & ANCHOR LAYOUT
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MANUFACTURER:

NABCO

DOOR PTVOT DOOR PIVOT GYRO TECH

N STRIKE STILE END $82 W18717 GEMINI DRIVE
5/8" TYP. STILE END P.0. BOX 906 MUSKEGO,

ROD ENGAGEMENT WISCONSIN 53150
PHONE: (877) 622-2694

V2222 2 2 E e T Z T ZT T2 22 72T 72 27 FAX: (262) 679-2505

. 1/4-20X3/4"
46" TYP. MOUNTING SCREWS

(954) 744-4738

KAWNEER #37227

FLUSH BOLTS TOP RAIL

DANIA BEACH, FL 33004

DOOR HARDWARE DETAILS
(954) 399-8478

-~ 1313
ADAMS RITE
LOCK W/ BOLTS

2

SYSTEM GT 1175 AUTO. SLIDER
398 E. DANIA BEACH BLVD. #338

o)
BUILDING DROPS, INC.

TITLE:
PREPARED BY:

/ STRIKE STILE END DETAIL

oo
L5 |9.2815 |

KAWNEER #37227
FLUSH BOLTS

HEADER

OPERATOR DRIVE
SHAFT WELDMENT

REVISIONS

DESCRIPTION

DOOR PIVOT DOOR PIVOT
STRIKE STILE END STILE END GUIDE CHANNEL

5TH EDITION FBC REVISIONS

1/4-20X3/4"
MOUNTING SCREWS

=
[ 4 |

DOOR HARDWARE DETAIL

NOTE:
— TOP RAIL
KAWNEER #37227 FLUSH BOLTS MAY BE SUBSTITUTED
W/ADAM'S RITE 1870 CYLINDER ACTIVATED BOLTS, TOP
&BOTTOM.

HERMES ¥, NORERO, P.E.
FLORIDA P, E, NO, 73778
398 EAST DANIA BEACH BLVD.
DANIA BEACH, FL 33004

PE CERT. OF AUTHORIZATION NO. 29578

DOOR PIVOT STILE END DETAIL
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MANUFACTURER:

INSTALLATION ANCHORS
SEE SHEET 2 FOR NABCO

QTY. AND SPACING
GYRO TECH

$82 W18717 GEMIN| DRIVE
P.0. BOX 906 MUSKEGO,

G WISCONSIN 53150
\ PERIMETER PHONE: (877) 622-2604
SEALANT FAX: (262) 679-2505
MAX. 1/4" SHIM

(954) 744-4738

HEADER

SEE GLAZING
DETAIL SHEET 6

$

MAX.DLO
7115/16"
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I\ ‘
EXTERIOR X / INTERIOR

VERTICAL SECTIONS
DANIA BEACH, FL 33004

SYSTEM 6T 1175 AUTO. SLIDER
(954) 399-8478

TITLE:
PREPARED BY:
0}
BUILDING DROPS, INC.
398 E. DANTIA BEACH BLVD. #338

Ls|o2815 |
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TOP RAIL

5TH EDITION FBC REVISIONS
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INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

. VERTICAL SECTION
“ SILL

MAX.DLO
7115/16"

DANIA BEACH, FL 33004

PE CERT. OF AUTHORIZATION NO. 20578

HERMES F. NOREROQ, P.E.
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD.

. VERTICAL SECTION
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MANUFACTURER:

INSTALLATION ANCHORS WEATHERING PILE N A B C o
SEE SHEET 2 FOR INTERIOR (SCHELEGEL POLYBOND) e

QTY. AND SPACING GYRO TECH
S$82 W18717 GEMIN| DRIVE
HINGE TUBE

P.0. BOX 906 MUSKEGO,
SEE|GLAZING WISCONSIN 53150
WEATHERING BULB KAWNEER DETAIL SHEET 6 PHONE: (877) 622-2694
FLUSH BOLTS FAX: (262) 679-2505
PIVOT STILE END ——/_

SEE DETAIL SHEET 3 \\

(954) 744-4738

HORIZONTAL SECTIONS
BUILDING DROPS, INC.
DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM GT 1175 AUTO. SLIDER

STRIKE STILE
EXTERIOR. END PIVOT

(SEE SHEET 3 FOR

DETAILS)

398 E. DANIA BEACH BLVD. #338

TITLE:

i0)

EXTERIOR

WAX. 1/4" SHIM HORIZONTAL SECTION .HORlZONTAL SECTION
: IAMB 5/ PANEL INTERLOCK

INTERIOR INTERIOR —INSTALLATION ANCHORS
SEE SHEET 2 FOR
QTY. AND SPACING

BY | DATE

z
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B
o
=
o
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w
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ARLOCK W/ BOLTS LOCK REINF. PLATES WEATHERING BULB

SEE GLAZING SEE SHEET 7 FOR
DETAIL SHEET 6 DETAILS AR LOCK
W/ BOLT

0
Z
o
=
%))
=
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o

A | 5TH EDITION FBC REVISIONS LS |9.28.15 | PREPARED BY:

WEATHERING BULB

DANIA BEACH, FL 33004
BPE CERT. OF AUTHORIZATION NO. 20578

HERMES F, NORERO, P.E,
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD,

EXTERIOR EXTERIOR MAX. 1/4" SHIM

E E }HORIZONTAL SECTION EE;HORIZONTAL SECTION
PANEL BUTT STILE JAMB

CHK BY:
HFN
SCALE:
NTS
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MANUFACTURER:

BILL OF MATERIALS NABCO
HEADER ITEM NO. DESCRIPTION MATERIAL NABCO PART NO. | MANUFACTURER |
. = 2aeotz ~GvROTECH
6063-T6 HEADER 6063-T6 W.L. BONNEL CO GYRO TECH
GUIDE CHANNEL 6063-T5 248913 W.L. BONNEL €O. $52 W18717 GEMIN| DRIVE
P.0. BOX 906 MUSKEGO,
HEADER DRESS PLATE 6063-T5 240129 W.L. BONNEL €O. WISGONSIN 53150
HINGE TUBE 6063-T5 148957 W.L. BONNEL €O PHONE: (877) 622-2694
FAX: (262) 679-2505
4" STILE 6063-T6 1413289 W.L. BONNEL €O

¢ 0170 ‘*

Gme | werw 14552 |WL BONNEL CO

(954) 744-4738

aacoe | wwe | wetes | -

TOP & BOTTOM RAIL DOOR 6063-T6 149085 W.L. BONNE|

e | |
<o
& [wmeson | ewsm | wsow [wesowecol
5 [vmeswowmaw | oosrs | 9ot we soweLcol
|
o)

DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM GT 1175 AUTO, SLIDER
B.O.M. COMPONENTS & 6LAZING
BUILDING DROPS, INC.
398 E. DANIA BEACH BLVD. #338

i0)

BY | DATE

—»‘ ‘—7 5/16" TEMPERED GLASS

EXTERIOR
12 INTERIOR

—GLASS %" x %" x %" ALUMINUM
; ) BITE " REINFORCEMENT ANGLE

@GUIDE CHANNEL HEADER DRESS PLATE / \®
6063-T5 6063-T5 DOW 995
STRUCTURAL
- 1810 —=— SILICONE

REVISIONS

DESCRIPTION

A | 5TH EDITION FBC REVISIONS |[LS |9.28.15 | PREPARED BY:

0.320
r #10-24X1 PFH SCREW
N THREAD FORMING AT 6"0C
—2" FROM ENDS

#10-24X2" PFH SCREW
THREAD FORMING AT 12"0C
GLAZING DETAIL 1 AND 3" OC NEAR THE CORNERS

HERMES F, NORERO, P.E,
FLORIDA P. E. NO. 73778
398 EAST DANIA BEACH BLVD,

DANIA BEACH, FL 33004
PE CERT, OF AUTHORIZATION NO. 29578

NOTE:

1) GLASS THICKNESS AND TYPE COMPLIES WITH
ASTM E 1300-04 6LASS CHART REQUIREMENTS.

2) ALL GLAZING CONFIGURATIONS SHALL COMPLY
WITH SAFETY GLAZING REQUIREMENTS
OUTLINED IN FBC SECTION 2406.

3)  MAX.DLO=15%" x 71"
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HINGE TUBE
6063-T5

21500 \‘« 0.130

THRESHOLD RAMP
6005-T5

—] 1250 |=—

0.500

?

(1)

‘—— 2.000 —= —

JAMB EXTENSION

4" STILE STILE
6063-T6 6063-T6

|

2.130
j‘» —~—0.090

‘—— 1750 ——‘

‘« 1.750 »‘

GLASS STOP CHANNEL

]

1.000

i

INTERIOR

AR 4066

THUMBTURN
ADAMS RITE AR 1853A/505
MAXIMUM SECURLTY LOCK
EXTENDING INTO HEADER
AND THRESHOLD

LOCK REINFORCEMENT PLATE
11/2X 15" X .105"
12 GAUGE STEEL

AR 4036 CYLINDER

STANDARD LOCK DETAIL

|
00
i

TOP & BOTTOM RAIL DOOR e THRESHOLD
6063-T6 6005-T5

0090 —=|=—

1

Y

- 1750 ]

GLASS STOP BASE REINF. ANGLE @ TRACK PLUG
6063-T5 6063-T5

0715 045 —m|f=—

6061-T6 RPVC

0.750 ——»‘

|

i+
01430 J 0.750

INTERIOR

AR 4550
MS DEADBOLT LEVER

ADAMS RITE AR 1853A/505
MAXIMUM SECURITY LOCK
EXTENDING INTO HEADER

AND THRESHOLD

[SEEERRRH TR

LOCK REINFORCEMENT PLATE
11/2X 15" X .105"
12 GAUGE STEEL

AR 4036 CYLINDER

ALTERNATE LOCK DETAIL

MANUFACTURER:

NABCO

GYRO TECH

582 W18717 GEMINI DRIVE
P.0. BOX 906 MUSKEGO,
WISCONSIN 53150
PHONE: (877) 622-2694
FAX: (262) 679-2505

(954) 744-4738

COMPONENTS
DANIA BEACH, FL 33004

(954) 399-8478

SYSTEM 6T 1175 AUTO. SLIDER

[0)
BUILDING DROPS, INC.
398 E. DANIA BEACH BLVD. #338

TITLE:
9.28.15 | PREPARED BY:
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REVISIONS
DESCRIPTION
5TH EDITION FBC REVISIONS

=
B

DANIA BEACH, FL 33004
PE CERT, OF AUTHORIZATION NO, 29578

HERMES ¥, NORERO, P.E.
FLORIDA P, E, NO. 73778
398 EAST DANIA BEACH BLVD.





